**8 BIT SUBSTRACTION:**

**CODE:**

LDA 2001

MOV B,A

LDA 2005

SUB B

STA 2010

HLT

**OUTPUT:**

